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1. Block
· Factory GM OEM blocks allowed. 
	Part Number
	Mfg
	Material
	Displacement
	Max Bore

	GMP12673475
	GM Performance
	Iron
	6.0 L
	4.030”



· Block lightening of any kind is not allowed. All mounts must remain. This includes fuel
pump, motor mounts, and all other stock mounts.
· Oversized and roller cam bearings are not allowed.

2. Crankshaft
· Stroke length must be  3.622” +/-0.005”.  
· No lightening, counterweight knife edging, or counterweight polishing is allowed. Balancing is allowed.
3. Connecting Rods
· Connecting rod length must be 6.098-6.125.
· Connecting rods and bolts must be magnetic steel.

4. Pistons/Rings
· Any forged or cast aluminum piston is allowed. 
· Engines must not exceed 12.3:1 compression ratio with the heads and gasket installed. 

5. Valvetrain
· Only hydraulic lifters with .700" OEM diameter roller wheel and .842 diameter are allowed.
· Push rods must be a stock, or stock type replacement, with a 5/16” diameter.
· Roller tip rockers are not allowed.
· Rockers must be 1.7:1 ratio.
· Maximum lift at the valve is .600”.

6. Cylinder Heads
· Only the following unmodified cylinder heads per manufacture’s specification are allowed. 
	Part Number
	Mfg
	Intake Valve Dia.
	Exhaust Valve Dia.
	Chamber CC
	Intake Port Volume CC
	Casting #

	88958758
	GM Performance
	2.165
	1.59
	70
	276
	821, 823



· Angle milling, material removal or addition in any area of head is not allowed.
· No porting, grinding or polishing of any kind is allowed.
· The seats and guides may be replaced.
· Valve springs must be magnetic steel.  
· Valve spring retainer may be steel or titanium.
7. Intake: Naturally aspirated induction only.  Turbo charging or super charging is not allowed.  
7a. GM Performance intake manifold Part Number 25534401
7b. Holley Part Number 300-131
7c. Edelbrock Victor Jr. Part Number 28457
7d. Edelbrock Super Victor Part Number 28265
· No modifications are allowed. 
· No porting, polishing, or grinding of any kind is allowed.
8. Fuel Delivery System
 	4 Barrel Carburetor: Spec Holley 750 cfm. The only allowed changes are jetting, 
power valves, and air bleeds. No other modifications are allowed. Carburetor 
will be subject to 1.375” venturi Go / no-Go gauge checking as part of tech. 

9. Fuel
· Racing methanol only. Gasoline is not allowed.
· Nitro, nitrous oxide, or any other oxidizer, with the exception of methanol, is not allowed.
· No fuel additives, other than upper cylinder lubricants, are allowed. Fuel is subject to inspection at any time.

10. Oiling System
· Wet sump oil pan reservoir system is required.
· OEM type pump, mechanically driven from crankshaft snout, is required. 
11. Ignition
Electronic Spark-only control of OE style coils on plug
· An MSD #6010, MSD #6014, MSD #6014CT or MSD #60143 ignition controller is required. 
· Only OE or physically compatible OE replacement coil packs are allowed.
· Only nominal 12V lithium-ion, Iron-phosphate, or NMC batteries are allowed. The battery must be securely hard mounted and shielded in the same area designated for ballast mounting.  Bus voltage must read less than 14.8 V at any time.
· On board starters are not allowed. 
· No electronic traction control devices are allowed.
· The ignition firing order must remain stock.
12. Exhaust: 
· Headers with maximum 1-3/4 tube diameter per cylinder, up to collector are required.
· Schoenfeld 14272735‑78 Muffler is the only muffler allowed.
· Tri Y headers are not allowed.
13. Water Pump & Radiator
· Any mechanically driven water pump is allowed.
· Electric water pumps are not allowed.
14. Fuel Pump
· A mechanical, belt driven, or cam driven fuel pump is allowed. 
· Electric fuel pumps are not allowed.
15. Exotic Materials
· No Titanium, Inconel, Ceramics, DLC, or Nikasil components are allowed.
